**Liberty University**

**CSIS 331**

**Lab 1 Answer Sheet**

**On Switch S1 type and press Enter.**

S1# **copy running-config startup-config**

S1# **show running-config**

Copy and paste Switch S1 Config Here.

S1#show running-config

Building configuration...

Current configuration : 1249 bytes

!

version 12.2

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

!

hostname S1

!

enable secret 5 $1$mERr$ILwq/b7kc.7X/ejA4Aosn0

enable password 7 08221D0A0A49

!

!

!

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

interface FastEthernet0/1

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface GigabitEthernet0/1

!

interface GigabitEthernet0/2

!

interface Vlan1

no ip address

shutdown

!

banner motd ^CThis is a secure system. Authorize Access Only!^C

!

!

!

line con 0

password 7 082D495A041C0C19

login

!

line vty 0 4

login

line vty 5 15

login

!

!

!

!

end

**On Switch S2 type and press Enter.**

S2# **copy running-config startup-config**

S2# **show running-config**

Copy and paste Switch S2 Config Here.

S2#show running-config

Building configuration...

Current configuration : 1323 bytes

!

version 12.2

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

!

hostname S2

!

enable secret 5 $1$mERr$ILwq/b7kc.7X/ejA4Aosn0

enable password 7 08221D0A0A49

!

!

!

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

interface FastEthernet0/1

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface GigabitEthernet0/1

!

interface GigabitEthernet0/2

!

interface Vlan1

no ip address

shutdown

!

banner motd ^CAuthorized access only. Unauthorized access is prohibited and violators will be prosecuted to the full extent of the law.^C

!

!

!

line con 0

password 7 082D495A041C0C19

login

!

line vty 0 4

login

line vty 5 15

login

!

!

!

!

end