**Liberty University**

**CSIS 331**


**Lab 12 Instructions**

**\*\*\*Please use the Topology and Instructions below to create a Packet Tracer from scratch. There will not be a Packet Tracer provided for you, you must create it new. If the routers do not have enough interfaces; you will need to go to the physical tab of the router and add the correct interface card to the existing router. Make sure the router is powered down while this is going on. Please reach out to your instructor if you have issues.\*\*\***

**Packet Tracer:**

*[Adapted from Cisco Networking Academy Routing and Switching 6.2.2.5]*

**Topology**



**Addressing Table**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Device** | **Interface** | **IP Address** | **Subnet Mask** | **Default Gateway** |
| S1 | VLAN 1 | 192.168.1.11 | 255.255.255.0 | N/A |
| S2 | VLAN 1 | 192.168.1.12 | 255.255.255.0 | N/A |
| PC-A | NIC | 192.168.10.3 | 255.255.255.0 | 192.168.10.1 |
| PC-B | NIC | 192.168.10.4 | 255.255.255.0 | 192.168.10.1 |
| PC-C | NIC | 192.168.20.3 | 255.255.255.0 | 192.168.20.1 |

**Objectives**

**Part 1: Build the Network and Configure Basic Device Settings**

**Part 2: Create VLANs and Assign Switch Ports**

**Part 3: Maintain VLAN Port Assignments and the VLAN Database**

**Part 4: Configure an 802.1Q Trunk between the Switches**

**Part 5: Delete the VLAN Database**

**Background / Scenario**

Modern switches use virtual local-area networks (VLANs) to improve network performance by separating large Layer 2 broadcast domains into smaller ones. VLANs can also be used as a security measure by controlling which hosts can communicate. In general, VLANs make it easier to design a network to support the goals of an organization.

VLAN trunks are used to span VLANs across multiple devices. Trunks allow the traffic from multiple VLANS to travel over a single link, while keeping the VLAN identification and segmentation intact.

In this lab, you will create VLANs on both switches in the topology, assign VLANs to switch access ports, verify that VLANs are working as expected, and then create a VLAN trunk between the two switches to allow hosts in the same VLAN to communicate through the trunk, regardless of which switch the host is actually attached to.

.

**Part 1: Build the Network and Configure Basic Device Settings**

In Part 1, you will set up the network topology and configure basic settings on the PC hosts and switches.

**Step 1: Cable the network as shown in the topology.**

Attach the devices as shown in the topology diagram, and cable as necessary.

**Step 2: Configure basic settings for each switch.**

a. Console into the switch and enter global configuration mode.

b. Copy the following basic configuration and paste it to the running-configuration on the switch.

no ip domain-lookup

service password-encryption

enable secret class

banner motd #

Unauthorized access is strictly prohibited. #

line con 0

password cisco

login

logging synchronous

line vty 0 15

password cisco

logging synchronous

login

exit

c. Configure the host name as shown in the topology.

d. Configure the IP address listed in the Addressing Table for VLAN 1 on the switch.

e. Administratively deactivate all unused ports on the switch.

f. Copy the running configuration to the startup configuration.

**Step 3: Configure PC hosts.**

Refer to the Addressing Table for PC host address information.

**Step 4: Test connectivity.**

Verify that the PC hosts can ping one another.

**Answer Ping Table on Answer Sheet.**

**Part 2: Create VLANs and Assign Switch Ports**

In Part 2, you will create student, faculty, and management VLANs on both switches. You will then assign the VLANs to the appropriate interface. The **show vlan** command is used to verify your configuration settings.

**Step 1: Create VLANs on the switches.**

a. Create the VLANs on S1.

S1(config)# **vlan 10**

S1(config-vlan)# **name Student**

S1(config-vlan)# **vlan 20**

S1(config-vlan)# **name Faculty**

S1(config-vlan)# **vlan 99**

S1(config-vlan)# **name Management**

S1(config-vlan)# **end**

b. Create the same VLANs on S2.

c. Issue the **show vlan** command to view the list of VLANs on S1.

S1# **show vlan**

VLAN Name Status Ports

---- -------------------------------- --------- -------------------------------

1 default active Fa0/1, Fa0/2, Fa0/3, Fa0/4

Fa0/5, Fa0/6, Fa0/7, Fa0/8

Fa0/9, Fa0/10, Fa0/11, Fa0/12

Fa0/13, Fa0/14, Fa0/15, Fa0/16

Fa0/17, Fa0/18, Fa0/19, Fa0/20

Fa0/21, Fa0/22, Fa0/23, Fa0/24

Gi0/1, Gi0/2

10 Student active

20 Faculty active

99 Management active

1002 fddi-default act/unsup

1003 token-ring-default act/unsup

1004 fddinet-default act/unsup

1005 trnet-default act/unsup

VLAN Type SAID MTU Parent RingNo BridgeNo Stp BrdgMode Trans1 Trans2

---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------

1 enet 100001 1500 - - - - - 0 0

10 enet 100010 1500 - - - - - 0 0

20 enet 100020 1500 - - - - - 0 0

99 enet 100099 1500 - - - - - 0 0

VLAN Type SAID MTU Parent RingNo BridgeNo Stp BrdgMode Trans1 Trans2

---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------

1002 fddi 101002 1500 - - - - - 0 0

1003 tr 101003 1500 - - - - - 0 0

1004 fdnet 101004 1500 - - - ieee - 0 0

1005 trnet 101005 1500 - - - ibm - 0 0

Remote SPAN VLANs

------------------------------------------------------------------------------

Primary Secondary Type Ports

------- --------- ----------------- ------------------------------------------

**Answer Questions 1 and 2 on the answer sheet.**

**Step 2: Assign VLANs to the correct switch interfaces.**

a. Assign VLANs to the interfaces on S1.

1) Assign PC-A to the Student VLAN.

S1(config)# **interface f0/6**

S1(config-if)# **switchport mode access**

S1(config-if)# **switchport access vlan 10**

2) Move the switch IP address VLAN 99.

S1(config)# **interface vlan 1**

S1(config-if)# **no ip address**

S1(config-if)# **interface vlan 99**

S1(config-if)# **ip address 192.168.1.11 255.255.255.0**

S1(config-if)# **end**

b. Issue the **show vlan brief** command and verify that the VLANs are assigned to the correct interfaces.

S1# **show vlan brief**

VLAN Name Status Ports

---- -------------------------------- --------- -------------------------------

1 default active Fa0/1, Fa0/2, Fa0/3, Fa0/4

Fa0/5, Fa0/7, Fa0/8, Fa0/9

Fa0/10, Fa0/11, Fa0/12, Fa0/13

Fa0/14, Fa0/15, Fa0/16, Fa0/17

Fa0/18, Fa0/19, Fa0/20, Fa0/21

Fa0/22, Fa0/23, Fa0/24, Gi0/1

Gi0/2

10 Student active Fa0/6

20 Faculty active

99 Management active

1002 fddi-default act/unsup

1003 token-ring-default act/unsup

1004 fddinet-default act/unsup

1005 trnet-default act/unsup

c. Issue the **show ip interface brief** command.

Answer questions 3 and 4 on the answer sheet.

d. Use the Topology to assign VLANs to the appropriate ports on S2.

e. Remove the IP address for VLAN 1 on S2.

f. Configure an IP address for VLAN 99 on S2 according to the Addressing Table.

g. Use the **show vlan brief** command to verify that the VLANs are assigned to the correct interfaces.

S2# **show vlan brief**

VLAN Name Status Ports

---- -------------------------------- --------- -------------------------------

1 default active Fa0/1, Fa0/2, Fa0/3, Fa0/4

Fa0/5, Fa0/6, Fa0/7, Fa0/8

Fa0/9, Fa0/10, Fa0/12, Fa0/13

Fa0/14, Fa0/15, Fa0/16, Fa0/17

Fa0/19, Fa0/20, Fa0/21, Fa0/22

Fa0/23, Fa0/24, Gi0/1, Gi0/2

10 Student active Fa0/11

20 Faculty active Fa0/18

99 Management active

1002 fddi-default act/unsup

1003 token-ring-default act/unsup

1004 fddinet-default act/unsup

1005 trnet-default act/unsup

**Answer questions 5 through 8 on the answer sheet.**

**Part 3: Maintain VLAN Port Assignments and the VLAN Database**

In Part 3, you will change VLAN assignments to ports and remove VLANs from the VLAN database.

**Step 1: Assign a VLAN to multiple interfaces.**

a. On S1, assign interfaces F0/11 – 24 to VLAN 10.

S1(config)# **interface range f0/11-24**

S1(config-if-range)# **switchport mode access**

S1(config-if-range)# **switchport access vlan 10**

S1(config-if-range)# **end**

b. Issue the **show vlan brief** command to verify VLAN assignments.

c. Reassign F0/11 and F0/21 to VLAN 20.

d. Verify that VLAN assignments are correct.

**Step 2: Remove a VLAN assignment from an interface.**

a. Use the **no switchport access vlan** command to remove the VLAN 10 assignment to F0/24.

S1(config)# **interface f0/24**

S1(config-if)# **no switchport access vlan**

S1(config-if)# **end**

b. Verify that the VLAN change was made.

**Answer question 9 in the answer sheet.**

**Step 3: Remove a VLAN ID from the VLAN database.**

a. Add VLAN 30 to interface F0/24 without issuing the VLAN command.

S1(config)# **interface f0/24**

S1(config-if)# **switchport access vlan 30**

% Access VLAN does not exist. Creating vlan 30

**Note**: Current switch technology no longer requires that the **vlan** command be issued to add a VLAN to the database. By assigning an unknown VLAN to a port, the VLAN adds to the VLAN database.

b. Verify that the new VLAN is displayed in the VLAN table.

S1# **show vlan brief**

VLAN Name Status Ports

---- -------------------------------- --------- -------------------------------

1 default active Fa0/1, Fa0/2, Fa0/3, Fa0/4

Fa0/5, Fa0/6, Fa0/7, Fa0/8

Fa0/9, Fa0/10, Gi0/1, Gi0/2

10 Student active Fa0/12, Fa0/13, Fa0/14, Fa0/15

Fa0/16, Fa0/17, Fa0/18, Fa0/19

Fa0/20, Fa0/22, Fa0/23

20 Faculty active Fa0/11, Fa0/21

30 VLAN0030 active Fa0/24

99 Management active

1002 fddi-default act/unsup

1003 token-ring-default act/unsup

1004 fddinet-default act/unsup

1005 trnet-default act/unsup

**Answer question 10 on the Answer Sheet.**

c. Use the **no vlan 30** command to remove VLAN 30 from the VLAN database.

S1(config)# **no vlan 30**

S1(config)# **end**

d. Issue the **show vlan brief** command. F0/24 was assigned to VLAN 30.

**Answer questions 11 and 12 on the Answer Sheet.**

S1# **show vlan brief**

VLAN Name Status Ports

---- -------------------------------- --------- -------------------------------

1 default active Fa0/1, Fa0/2, Fa0/3, Fa0/4

Fa0/5, Fa0/6, Fa0/7, Fa0/8

Fa0/9, Fa0/10, Gi0/1, Gi0/2

10 Student active Fa0/12, Fa0/13, Fa0/14, Fa0/15

Fa0/16, Fa0/17, Fa0/18, Fa0/19

Fa0/20, Fa0/22, Fa0/23

20 Faculty active Fa0/11, Fa0/21

99 Management active

1002 fddi-default act/unsup

1003 token-ring-default act/unsup

1004 fddinet-default act/unsup

1005 trnet-default act/unsup

e. Issue the **no switchport access vlan** command on interface F0/24.

f. Issue the **show vlan brief** command to determine the VLAN assignment for F0/24.

**Answer questions 13 on the Answer Sheet.**

**Note**: Before removing a VLAN from the database, it is recommended that you reassign all the ports assigned to that VLAN.

**Answer question 14 on the Answer Sheet.**

**Part 4: Configure an 802.1Q Trunk Between the Switches**

In Part 4, you will configure interface F0/1 to use the Dynamic Trunking Protocol (DTP) to allow it to negotiate the trunk mode. After this has been accomplished and verified, you will disable DTP on interface F0/1 and manually configure it as a trunk.

**Step 1: Use DTP to initiate trunking on F0/1.**

The default DTP mode of a 2960 switch port is dynamic auto. This allows the interface to convert the link to a trunk if the neighboring interface is set to trunk or dynamic desirable mode.

a. Set F0/1 on S1 to negotiate trunk mode.

S1(config)# **interface f0/1**

S1(config-if)# **switchport mode dynamic desirable**

\*Mar 1 05:07:28.746: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan1, changed state to down

\*Mar 1 05:07:29.744: %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/1, changed state to down

S1(config-if)#

\*Mar 1 05:07:32.772: %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/1, changed state to up

S1(config-if)#

\*Mar 1 05:08:01.789: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan99, changed state to up

\*Mar 1 05:08:01.797: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan1, changed state to up

You should also receive link status messages on S2.

S2#

\*Mar 1 05:07:29.794: %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/1, changed state to down

S2#

\*Mar 1 05:07:32.823: %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/1, changed state to up

S2#

\*Mar 1 05:08:01.839: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan99, changed state to up

\*Mar 1 05:08:01.850: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan1, changed state to up

b. Issue the **show vlan brief** command on S1 and S2. Interface F0/1 is no longer assigned to VLAN 1. Trunked interfaces are not listed in the VLAN table.

S1# **show vlan brief**

VLAN Name Status Ports

---- -------------------------------- --------- -------------------------------

1 default active Fa0/2, Fa0/3, Fa0/4, Fa0/5

Fa0/24, Gi0/1, Gi0/2

10 Student active Fa0/6, Fa0/12, Fa0/13, Fa0/14

Fa0/15, Fa0/16, Fa0/17, Fa0/18

Fa0/19, Fa0/20, Fa0/22, Fa0/23

20 Faculty active Fa0/11, Fa0/21

99 Management active

1002 fddi-default act/unsup

1003 token-ring-default act/unsup

1004 fddinet-default act/unsup

1005 trnet-default act/unsup

c. Issue the **show interfaces trunk** command to view trunked interfaces. Notice that the mode on S1 is set to desirable, and the mode on S2 is set to auto.

S1# **show interfaces trunk**

Port Mode Encapsulation Status Native vlan

Fa0/1 desirable 802.1q trunking 1

Port Vlans allowed on trunk

Fa0/1 1-4094

Port Vlans allowed and active in management domain

Fa0/1 1,10,20,99

Port Vlans in spanning tree forwarding state and not pruned

Fa0/1 1,10,20,99

S2# **show interfaces trunk**

Port Mode Encapsulation Status Native vlan

Fa0/1 auto 802.1q trunking 1

Port Vlans allowed on trunk

Fa0/1 1-4094

Port Vlans allowed and active in management domain

Fa0/1 1,10,20,99

Port Vlans in spanning tree forwarding state and not pruned

Fa0/1 1,10,20,99

**Note**: By default, all VLANs are allowed on a trunk. The **switchport trunk** command allows you to control

what VLANs have access to the trunk. For this lab, keep the default settings which allows all VLANs to traverse F0/1.

d. Verify that VLAN traffic is traveling over trunk interface F0/1**. Complete the second ping table on the Answer Sheet.**

**Step 2: Manually configure trunk interface F0/1.**

The **switchport mode trunk** command is used to manually configure a port as a trunk. This command should be issued on both ends of the link.

a. Change the switchport mode on interface F0/1 to force trunking. Make sure to do this on both switches.

S1(config)# **interface f0/1**

S1(config-if)# **switchport mode trunk**

b. Issue the **show interfaces trunk** command to view the trunk mode. Notice that the mode changed from **desirable** to **on**.

S2# **show interfaces trunk**

Port Mode Encapsulation Status Native vlan

Fa0/1 on 802.1q trunking 99

Port Vlans allowed on trunk

Fa0/1 1-4094

Port Vlans allowed and active in management domain

Fa0/1 1,10,20,99

Port Vlans in spanning tree forwarding state and not pruned

Fa0/1 1,10,20,99

**Answer question 15 on the Answer Sheet.**

**Part 5: Delete the VLAN Database**

In Part 5, you will delete the VLAN Database from the switch. It is necessary to do this when initializing a switch back to its default settings.

**Step 1: Determine if the VLAN database exists.**

Issue the **show flash** command to determine if a **vlan.dat** file exists in flash.

S1# **show flash**

Directory of flash:/

3 -rwx 43032 Mar 1 1993 00:01:24 +00:00 multiple-fs

4 -rwx 5 Mar 1 1993 00:01:24 +00:00 private-config.text

5 -rwx 11607161 Mar 1 1993 02:37:06 +00:00 c2960-lanbasek9-mz.150-2.SE.bin

6 -rwx 736 Mar 1 1993 00:19:41 +00:00 vlan.dat

32514048 bytes total (20858880 bytes free)

**Note**: If there is a **vlan.dat** file located in flash, then the VLAN database does not contain its default settings.

**Step 2: Delete the VLAN database.**

a. Issue the **delete vlan.dat** command to delete the vlan.dat file from flash and reset the VLAN database back to its default settings. You will be prompted twice to confirm that you want to delete the vlan.dat file. Press Enter both times.

S1# delete vlan.dat

Delete filename [vlan.dat]?

Delete flash:/vlan.dat? [confirm]

S1#

b. Issue the **show flash** command to verify that the vlan.dat file has been deleted.

S1# **show flash**

Directory of flash:/

2 -rwx 1285 Mar 1 1993 00:01:24 +00:00 config.text

3 -rwx 43032 Mar 1 1993 00:01:24 +00:00 multiple-fs

4 -rwx 5 Mar 1 1993 00:01:24 +00:00 private-config.text

5 -rwx 11607161 Mar 1 1993 02:37:06 +00:00 c2960-lanbasek9-mz.150-2.SE.bin

32514048 bytes total (20859904 bytes free)

**Answer Question 16 and the Reflection Questions on the Answer Sheet.**